TCP/IP Stack: Initialization Started
=== SD INIT START ===
=== SD INIT DONE ===

--- SDHC1 Pin Configuration ---
PORTB PMUX[9]  = 0x88
PORTB PMUX[10] = 0x88
PB18 PINCFG = 0x01
PB19 PINCFG = 0x01
PB20 PINCFG = 0x01
PB21 PINCFG = 0x01
PORTA PMUX[10] = 0x88
PA20 PINCFG = 0x01
PA21 PINCFG = 0x01
PORTD PMUX[10] = 0x08
PD20 PINCFG = 0x01
PD21 PINCFG = 0x06
--------------------------------
[SD DEBUG] PD20 (Card Detect) Level = 0
Device On

========== In createModbus() ==============

========== Exit createModbus() ==============

========== In createModbus() ==============
Creating Modbus TCP
  IP    :
  Port  : 0
  Slave : 1

========== Exit createModbus() ==============
MODBUS Config , 0, 0
Modbus connect ...
Is ModbusTCPConnected function
MBTCP: Creating socket to :0
MBTCP: Invalid IP
[SD DRIVER] Open succeeded. Handle=65536, ClientIndex=0

========== In createModbus() ==============

========== Exit createModbus() ==============

========== In createModbus() ==============
Creating Modbus TCP
  IP    :
  Port  : 0
  Slave : 1

========== Exit createModbus() ==============
MODBUS Config , 0, 0
Modbus connect ...
Is ModbusTCPConnected function
MBTCP: Creating socket to :0
MBTCP: Invalid IP
[SD] State: INIT -> WAIT
TX: AT
[EVENT TRIGGERED!] Event=0 Data='/mnt/myDrive1'
[SD EVENT] Mount: /mnt/myDrive1
[SD EVENT] Volume matched

[SD] Opening File: test.txt
[SD] File Open: SUCCESS
[SD] Writing Data...
[SD] Write SUCCESS
[SD] Reading File...
[SD] Read SUCCESS
[SD] Data: Elpis IT Solutions Pvt. Ltd.
